# ***ALL NEW***

#
Set Angle: Cmd 188

## Inputs

Offset | Description | Hex | Dec
0 | Command number | 00bc | 188
1 | Number of arguments | 0001 | 1
2 | Angle * 64 | xxxx | xxxx

## Description

This command sets the position of the Turntable shaft in the 8120 Chamber. It must be called from the Coupler Directional (38) screen.

This command is only available on the Fonix 8000 analyzer.

## Available in Modes

· Coupler Directional (38)

## Related Commands

Get Angle (189)