#
Coupler Directional (Major 38) Command List

These commands are available in the Coupler Directional screen (major mode 38). List of Common Commands contains a list of additional commands available in all modes of the hearing aid analyzer.

## Set Commands

Set Active Status (54)

Set Aid Selection (123)

Set Angle (188)

Set Automatic Mode (48)

Set Curve Frame (9)

Set Curve Group (182)

Set Ear Selection (75)

Set Filter Selection (136)

Set Frequency (2)

Set Gain Status (12)

Set List (118)

Set Measurement Delay (84)

Set Noise Reduction (4)

Set Option Parameters (70)

Set Selected Curve (112)

Set Source Amplitude (0)

Set Source Type (77)

Set Test State (59)

## Get Commands

Get Active Status (55)

Get Aid Selection (124)

Get Angle (189)

Get Automatic Mode (49)

Get Curve Frame (25)

Get Curve Group (183)

Get Ear Selection (76)

Get Filter Selection (137)

Get Frequency (23)

Get Gain Status (36)

Get List (119)

Get Measurement Delay (83)

Get Noise Reduction (26)

Get Option Parameters (71)

Get Selected Curve (113)

Get Source Amplitude (21)

Get Source Type (78)

Get Test State (60)