#
Set Option Parameters: Cmd 70

## Inputs

Offset | Description | Hex | Dec
0 | Command number | 0046 | 70
1 | Variable number of parameters | cccc | cccc
2 | Major state # | xxxx | xxxx
3-??? | Parameters according to state | yyyy | yyyy

## Description

This command is used to change settings used in automated test sequences such as ANSI, JIS, and IEC. The parameters input with this command vary depending upon the test screen. See the Major:Minor State topics for more details.

In order to use this command, you must be in the major state of the test sequence you wish to modify. For backwards compatibility reasons, the first parameter of the command is always the major state # of the current state. The parameters listed in the Major:Minor State topics follow this number.

## Available in Modes

· ANSI 87: Major Mode 2 (7000 only)

· IEC 94: Major Mode 3

· JIS: Major Mode 4

· ISI: Major Mode 5 (FP35 only)

· ANSI 92: Major Mode 12 (7000 only)

· ANSI 96: Major Mode 18

· ANSI 03: Major Mode 33

· IEC 05: Major Mode 37

· Coupler Directional: Major Mode 38

## Related Commands

Get Option Parameters (71)

Set Instrument State (59)

Get Instrument State (60)