#
Get List: Cmd 119

## Inputs

Offset | Description | Hex | Dec
0 | Command number | 0077 | 119
1 | Number of arguments | 0001 | 1
2 | List number to get | xxxx | xxxx

## Outputs

Offset | Description | Hex | Dec
0 | Acknowledgment of cmd 119 | 8077 | -32649
1 | Response (variable) | xxxx | xxxx

## Parameters - List Type

Description | Hex | Dec
Current measurement frequency list | 0000 | 0
Current distortion frequency list | 0001 | 1
Current user measurement frequency list | 0002 | 2
Current user distortion frequency list | 0003 | 3
Tone sweep settle list | 0004 | 4
I/O Sweep settle list | 0005 | 5
Get weighting of frequency bins | 0006 | 6
Get Polar Angle list | 0007 | 7
Set Polar Delay list | 0008 | 8

## Description

This command gets the selected list of data from the instrument. It can be used to read things such as the pure tone sweep frequency list or the Distortion frequency list.

The following parameters are available on the 7000:

· In the Coupler Multicurve screen, parameters 0, 1, and 4

· In the ANSI 87, ANSI 96, ANSI 03, JIS, IEC 94, IEC 05 screens, parameters 0, 4, and 5

· In the Insertion Gain and Real-ear SPL screens, parameters 0 and 4

· In the Visible Speech screen, parameter 6

On the 7000, this command is used in the Visible Speech screen to obtain the list of Speech Intelligibility Index (SII) coefficients. This is the weighting, in hundredths of a percent, of the frequency bins. These weights are used when computing the SII value.

On the 8000, this command is used in the Coupler Directional screen to:

Parameter 0: Get the Difference curve frequency list.

Parameter 4: Get the per frequency settling times for the Difference curve(if is is a tone curve).

Parameter 7: Get the list of Angles(times 64) used in the polar test.

Parameter 8: Get the list of Polar Settling times.

## Available in Modes

· Coupler (1)

· ANSI 87 (2) (7000, 8000 only)

· IEC 94 (3)

· JIS (4)

· Real-ear Insertion Gain (6)

· ANSI 96 (18)

· Real-ear SPL (23)

· Coupler Target (26) (FP35 only)

· Coupler EarSim (27) (FP35 only)

· ANSI 03 (33)

· IEC 05 (37) (7000, 8000 only)

· Visible Speech (36) (7000, 8000 only)

· Coupler Directional (38) (8000 only)

## Related Commands

Set List (118)

Do Custom Sweep (176)