#
Coupler Directional (Major 38) Parameters (8000 only)(ALL NEW)

The Set Option Parameters (70) and Get Option Parameters (71) commands are used in the Coupler Directional mode to set and obtain the parameters used in this screen. See the details below for each parameter.

Offset | Description | Hex | Dec
0 | Command number | 0046 | 70
1 | Number of arguments | 000b | 11
2 | Major state # | 0026 | 38
3 | Polar Test On/Off | xxxx | xxxx
4 | Polar Test Resolution | xxxx | xxxx
5 | Polar Plot Signal | xxxx | xxxx
6 | Polar Start Delay | xxxx | xxxx
7 | Polar Measurement Delay | xxxx | xxxx
8 | Diff Test On/Off | xxxx | xxxx
9 | Diff Curve Forward Angle | xxxx | xxxx
10 | Diff Curve Reverse Angle | xxxx | xxxx
11 | Diff Curve Start Delay | xxxx | xxxx
12 | Diff Curve Measurement Delay | xxxx | xxxx

## Polar Test On/Off

Description | Hex | Dec
Off | 0000 | 0
On | 0001 | 1

## Polar Test Resolution

Description | Hex | Dec
#Points from 2 to 361 | xxxx | xxxx

## Polar Plot Signal

Description | Hex | Dec
Auto | 0000 | 0
Continuous | 0001 | 1

## Polar Start&Measurement Delays

Description | Hex | Dec
Default | 0000 | 0
Specified | 0001-1388 | 1-5000

## Difference Test On/Off

Description | Hex | Dec
Off | 0000 | 0
On | 0001 | 1

## Difference Curve Forward/Reverse Angles

Description | Hex | Dec
Range 0 to 360 degrees |  |
Resolution 1/64th of a Degree |  |
0 degrees | 0000 | 0
1 degree | 0040 | 64
360 degrees | 5a00 | 23,040

## Difference Curve Start&Measurement Delays

Description | Hex | Dec
Default | 0000 | 0
Specified | 0001-1388 | 1-5000