#
Set Automatic Mode: Cmd 48

## Inputs

Offset | Description | Hex | Dec
0 | Command number | 0030 | 48
1 | Number of One or Two arguments | 0001 or 0002 | 1 or 2
2 | Automatic mode setting | xxxx | xxxx
3 | Auto Return(CD only) | xxxx | xxxx

## Parameters

Automatic Mode Description | Hex | Dec
Set Auto mode to OFF | 0000 | 0
Set Auto mode to Semi-Automatic | 0001 | 1
Set Auto mode to Fully-Automatic | 0002 | 2
Set Auto mode to Program | 0003 | 3
Set Auto mode to Simultaneous(CD only) | 0004 | 4

## Auto Return Mode(Coupler Directional screen only)

## Set curve back to 1 after running an automatic sequence (1-on or 0-off).

## Description

This command sets the automatic mode used in the Coupler Multicurve and Coupler Directional screens. If this command is called from the Default Settings mode (16), the global setting is changed, and the coupler screen local value will be changed to the new global setting upon the next entry to the coupler screen. If this command is called from the Coupler mode (1 or 38), however, the global setting is unchanged. The local coupler setting remains while in the Coupler screen, but the existing global setting will be reapplied if the coupler mode is exited and re-entered.

This command is not only available on the FP35 analyzer 7000 and 8000.

## Available in Modes

· Coupler (1)

· Coupler Directional (38)

· Default Settings Menu (16)

## Related Commands

Get Automatic Mode (49)

Set Curve Group (182)

Get Curve Group (183)