What is included with this distribution.

Fryers-Drivers:

This directory contains the Fryers driver files.
It also contains the documentation for programmers
on how the drivers work.

Note: The Fryers32.DLL and/or FryeCom.DLL must be 
installed either in the Windows System32 directory,
or in the directory location of the program that 
uses the DLL. If the file is located in the System32
directory, then all programs that require the DLL 
can share it (however, installing the file there 
may require administrator privleges).


Install-RS232:

This directory contains the documents on how to install
and troubleshoot RS232 interface on older Frye equipment 
so that they can be controlled via RS232. 


Legacy:

This directory contains the legacy Fryers programming 
documentation and source code for those that still are 
using the older drivers. 


Programming:

This directory contains examples and documentation for 
programming to the new FryeCom device driver used to
communicate with Fonix equipment. 


User-Tools:
This directory contains program tools for users to use
to collect data or test the operation of the Fonix 
instrument connected to a computer. 

Of particular interest are three programs, 

  FCapture:
    A Screen capture program used to capture the screen 
    display on a Fonix instrument. Useful for publishing 
    test results. 

  SetLabel:
    A program to configure the print label on Fonix 
    insturments with a built-in printer.

  FCheck: 
    A program to test the communication interface between
    a computer and the Fonix instrument. This program will
    tell you if the instrument is properly connected and
    operational and what COM port it is connected to 
    on the computer. 


<eof>
