                   Speed Bump Test For Fryers
                          07/11/97 -med

This program is used to stress the operation of the Fryers 
Driver. There are two versions, 16 and 32. The 16bit version 
uses the FRYERS.COM file to stress that driver. The 32 bit 
version uses the FRYERS32.DLL file to stress that version. 

Only the source code is provided, so if you want to use the 
program, you will have to have a 16 or 32 bit copy of Delphi to 
compile the code. This program is provided simply because it 
exists. It is used as a testing tool to stress the Fryers driver 
under various situations. It is mainly a development tool, and as 
such is incomplete. The software is adapted by the development 
engineer as need arises.

It is provided here mainly as a source reference. This program 
is not to be used as a full test of the Fryers driver since it 
does not provide such functionality.

<eof>


