

                    FA series Audiometer FIPP command summary
                                                            11/06/92 -med

        All standard FIPP instruments have these commands:
        =================================================================
                            Basic Common Command Set

        Command                                                    Number
        ----------------------------------------------------------------- 
        Get Version                                                    28
        Get Cmd Status                                                 33
        Do Reset                                                       38


        Response                                     (Command)     Number
        ----------------------------------------------------------------- 
        Version                                           (28)     -28644
        Cmd Status                                        (33)     -28639





        All FA1x series audiometers have these commands:
        =================================================================
                              Standard Command Set

        Command                                                    Number
        ----------------------------------------------------------------- 
        Get Control Registers                                           1
        Set Control Registers                                           2
        Get Keyboard Input Registers                                    9
        Get Calibration Flags                                          10
        Set Calibration Flags                                          11
        Get Calibration Data                                           12
        Set Calibration Data                                           13
        Do EEROM Read                                                  14 
        Do EEROM Write                                                 15


        Response                                     (Command)     Number
        ----------------------------------------------------------------- 
        Control Registers                                  (1)     -28671
        Keyboard Input Register Data                       (9)     -28663
        Calibration Flags                                 (10)     -28662
        Calibration Data                                  (12)     -28660











                                        1


        FA1x series with the standard RS232 option have this command set:
        =================================================================
                              Extended Command Set

        Command                                                    Number
        ----------------------------------------------------------------- 
        Get Patient Response Latched Control Registers                  3
        Get Patient Response Latch Counter                              4
        Get Front Panel Registers                                       5
        Get Buffered Front Panel Registers                              6
        Get Buffered Front Panel Counter                                7
        Get System Status Registers                                     8
        Do Patient Response Latch Array Flush                          31 
        Do Buffered Front Panel Array Flush                            32 
        Do Error                                                       34
        Set Level Boost Enable Flags                                   37
        Do Sleep                                                       39


        Response                                     (Command)     Number
        ----------------------------------------------------------------- 
        Patient Response Latched Control Registers         (3)     -28669
        Patient Response Latch Count                       (4)     -28668
        Front Panel Registers                              (5)     -28667
        Buffered Front Panel Registers                     (6)     -28666
        Buffered Front Panel Count                         (7)     -28665
        System Status Registers                            (8)     -28664


        =================================================================
                              Warble/Pulse Commands
        Command                                                    Number
        ----------------------------------------------------------------- 
        Get Warble/Pulse Control Registers                             18
        Set Warble/Pulse Control Registers                             19


        Response                                     (Command)     Number
        ----------------------------------------------------------------- 
        Warble\Pulse Control Registers                    (18)     -28654




        FA1x series with the ASCII RS232 option have this command set:
        =================================================================
                              ASCII Command Set

        Command                                                    Number
        ----------------------------------------------------------------- 
        Set ASCII Mode                                                 30






                                        2


        FA1x series with the standard RS232 option have this command set:
        =================================================================
                               Sequencer Commands

        Command                                                    Number
        ----------------------------------------------------------------- 
        Get Sequencer Data                                             20
        Set Sequencer Data                                             21
        Get Sequencer Index                                            22
        Set Sequencer Index                                            23
        Get Sequencer Enable                                           24
        Set Sequencer Enable                                           25
        Get Sequencer Control Array                                    26
        Get Sequencer Activity Information                             27


        Response                                     (Command)     Number
        ----------------------------------------------------------------- 
        Sequencer Data                                    (20)     -28652
        Sequencer Index                                   (22)     -28650
        Sequencer Enable flag                             (24)     -28648
        Sequencer Activity Information                    (27)     -28645



        FA1x series with the standard RS232 option have this command set:
        =================================================================
                           Special Debug/Test Commands

        Command                                                    Number
        ----------------------------------------------------------------- 
        Get I/O Port Image                                             29
        Get Warble Table                                               16 
        Set Warble Table                                               17


        Response                                     (Command)     Number
        ----------------------------------------------------------------- 
        Warble Table data                                 (16)     -28656
        Sequencer Control Array                           (26)     -28646
        I/O Port Image                                    (29)     -28643
















                                        3


        =================================================================
                         FA1x commands in numeric order

        Command                                                    Number
        ----------------------------------------------------------------- 

        <reserved>                                                      0  
        Get Control Panel Registers                                     1
        Set Control Panel Registers                                     2
        Get Patient Response Latched Control Registers                  3
        Get Patient Response Latch Counter                              4
        Get Front Panel Registers                                       5
        Get Buffered Front Panel Registers                              6
        Get Buffered Front Panel Counter                                7
        Get System Status Registers                                     8
        Get Keyboard Input Registers                                    9
        Get Calibration Flags                                          10
        Set Calibration Flags                                          11
        Get Calibration Data                                           12
        Set Calibration Data                                           13
        Do EEROM Read                                                  14 
        Do EEROM Write                                                 15
        Get Warble Table                                               16 
        Set Warble Table                                               17
        Get Warble/Pulse Control Registers                             18
        Set Warble/Pulse Control Registers                             19
        Get Sequencer Data                                             20
        Set Sequencer Data                                             21
        Get Sequencer Index                                            22
        Set Sequencer Index                                            23
        Get Sequencer Enable                                           24
        Set Sequencer Enable                                           25
        Get Sequencer Control Array                                    26
        Get Sequencer Activity Information                             27
        Get Version                                                    28
        Get I/O Port Image                                             29
        Set ASCII Mode                                                 30  
        Do Patient Response Latch Array Flush                          31 
        Do Buffered Front Panel Array Flush                            32 
        Get Cmd Status                                                 33
        Do Error                                                       34   
        <reserved>                                                     35   
        <reserved>                                                     36   
        Set Level Boost Enable Flags                                   37
        Do Reset                                                       38
        Do Sleep                                                       39











                                        4


        =================================================================
                         FA1x responses in numeric order

        Response                                     (Command)     Number
        ----------------------------------------------------------------- 
        Control Registers                                  (1)     -28671
        Patient Response Latched Control Registers         (3)     -28669
        Patient Response Latch Count                       (4)     -28668
        Front Panel Registers                              (5)     -28667
        Buffered Front Panel Registers                     (6)     -28666
        Buffered Front Panel Count                         (7)     -28665
        System Status Register data                        (8)     -28664
        Keyboard Input Register data                       (9)     -28663
        Calibration Flags                                 (10)     -28662
        Calibration data                                  (12)     -28660
        EEROM Read Status                                 (14)     -28658
        EEROM Write Status                                (15)     -28657
        Warble Table data                                 (16)     -28656
        Warble\Pulse Control Registers                    (18)     -28654
        Sequencer Data                                    (20)     -28652
        Sequencer Index                                   (22)     -28650
        Sequencer Enable flag                             (24)     -28648
        Sequencer Control Array                           (26)     -28646
        Sequencer Activity Information                    (27)     -28645
        Version                                           (28)     -28644
        I/O Port Image                                    (29)     -28643
        Cmd Status                                        (33)     -28639






























                                        5


        <eof>
























































                                        6
