#
Get Automatic Mode: Cmd 49

## Inputs

Offset | Description | Hex | Dec
0 | Command number | 0031 | 49
1 | Number of arguments | 0000 | 0

## Outputs

Offset | Description | Hex | Dec
0 | Acknowledgment of cmd 49 | 8031 | -32719
1 | One or Two word response | 0001 or 0002 | 1 or 2
2 | Automatic Mode status | xxxx | xxxx
3 | Auto Return Mode(CD only) | xxxx | xxxx

## Parameters

Automatic Mode Description | Hex | Dec
Auto mode is OFF | 0000 | 0
Auto mode is Semi-Automatic | 0001 | 1
Auto mode is Fully-Automatic | 0002 | 2
Set Auto mode to Program | 0003 | 3
Auto mode is Simultaneous(CD only) | 0004 | 4

## Auto Return Mode(Coupler Directional screen only)

## Set curve back to 1 after running an automatic sequence (1-on or 0-off).

## Description

This command requests the current status of the Automatic Mode. When called from the Default Settings mode (16), this command gets the global Auto Mode setting. When called from the Coupler Multicurve mode (1) or Coupler Directional (38), this command gets the local setting of the coupler screen.

This command is not supported only available on the FONIX FP35 analyzer 7000 and 8000.

## Available in Modes

· Coupler (1)

· Coupler Directional (38)

· Default Settings (16)

## Related Commands

Set Automatic Mode (48)