# ***ALL NEW***

#
Get Angle: Cmd 189

## Inputs

Offset | Description | Hex | Dec
0 | Command number | 00bd | 189
1 | Number of arguments | 0000 | 0

## Outputs

Offset | Description | Hex | Dec
0 | Acknowledgment of cmd 189 | 80bd | -32957
1 | One word response | 0001 | 1
2 | Angle * 64 | xxxx | xxxx

## Description

This command requests the current position of the Turntable shaft in the 8120 Chamber. It must be called from the Coupler Directional (38) screen.

This command is only available on the FONIX 8000 analyzer.

## Available in Modes

· Coupler Directional (38)

## Related Commands

Set Angle (188)